**Programming the MDH Auto-Dialler**

Notice: The system must be in the OFF mode for all programming:

To achieve this press **1**, **2**, **3**, **4**, **Esc**.

Recording the voice message

Press **1**, **2**, **3**, **4**, **Record**, **1**, **Enter.** When you have finished the message press **Enter** to stop recording. Note you have 30 seconds to record your message.

Playing the voice message

Press **1**, **2**, **3**, **4**, **Play**, **1**, **Enter.** This will play back the recorded message.

Programming in telephone numbers

Press **1**, **2**, **3**, **4**, **Program**, **3**, **Enter**, **1**, **Enter** <Telephone Number> **Enter**. You can enter a maximum of nine telephone numbers for the triggers. If you are using the dialer in an office, you maybe have to enter 9 before the number to get an outside line.

To enter in the second phone number, press **1**, **2**, **3**, **4**, **Program**, **3**, **Enter**, **2**, **Enter** <Telephone Number> **Enter**.

To enter in the third phone number, press **1**, **2**, **3**, **4**, **Program**, **3**, **Enter**, **3**, **Enter** <Telephone Number> **Enter**.

To enter in the fourth phone number, press **1**, **2**, **3**, **4**, **Program**, **3**, **Enter**, **4**, **Enter** <Telephone Number> **Enter**.

Keep repeating this to program in for nine channels for the relevant telephone numbers, the next sequence for the fifth number is **1**, **2**, **3**, **4**, **Program**, **3**, **Enter**, **5**, **Enter** <Telephone Number> **Enter**.

Deleting telephone numbers

Press **1**, **2**, **3**, **4**, **Program**, **3**, **Enter**, **1**, **Enter**, **Esc.**

To delete the second number would be **1, 2, 3, 4, Program, 3, Enter, 2, Enter, Esc** and so on for the third number **1, 2, 3, 4, Program, 3, Enter, 3, Enter, Esc.**

Programming the dialler to give a local audible alarm as well as sending voice message

Press **1, 2, 3, 4, Program, 1, Enter, 1, Enter.**

To turn off – Press **1, 2, 3, 4, Program, 1, Enter, 0, Enter.**

Designate telephone numbers to trigger one and two

Press **1**, **2**, **3**, **4**, **Program**, **6**, **Enter, 1, Enter,** (select/deselect numbers), **Enter –** Trigger One.

For trigger two.. Press **1**, **2**, **3**, **4**, **Program**, **6**, **Enter, 2, Enter,** (select/deselect numbers), **Enter.**

Turn the dialer on

When you have finished programming, activate the dialer by pressing **1**, **2**, **3**, **4**, **Enter.** Then the dialler is operational and ready for use.